RYK26004

|  |  |
| --- | --- |
|  | |
| Image Device | 1/3” Color CCD  Super HAD II  (Sony Chipset) effioA |
| Picture Elements | NTSC: 976x494  PAL: 976x582 |
| Resolution | 800TVL |
| Min Illumination | 0.01Lux/ F1.2 |
| S/N Ratio | More than 50dB |
| Electronic Shutter | NTSC: 1/60S~1/100,000S; PAL: 1/50S~1/100,000S |
| Gamma | 0.45 |
| Lens Furnished | 3.7mm lens |
| White Balance | Auto |
| Gain Control | Auto |
| Sync. System | Internal |
| Video Output | 1Vp-p/ 75 Ohms |
| Power Supply | DC 12V±10％ |
| Power  Consumption | 95mA |